**SECTION I – SPRAYERS, FOGGERS AND MISTERS**

**ITEM #1, BACKPACK SPRAYER, STORM ELECTRIC BACKPACK SPRAYER, AS SPECIFIED, OR EQUAL**

**COMPLIANCE**

**YES NO**

Heavy duty sprayer handle

4 Gallon Tank

Rechargeable 18 Volt Battery

58 PSI Operating Pressure

High and Low Flow Switch

40 Tanks per Charge

Includes Battery and Charger

**ITEM #2, BACKPACK SPRAYER, STIHL SR200, AS SPECIFIED, OR EQUAL**

Weight without liquid 18.7 Lbs.

Displacement 1.66 cubic inches

Engine Power 1.07 bhp

Engine 2 cycle

Fuel Capacity 36.5 oz.

Container Capacity 10.0 L

Air Volume, with tubes 580 m3/h

Air Velocity 181 mph

Maximum Spray Range Horizontal: 29.5 ft.; Vertical: 18 ft.

Warranty Two (2) Year Manufacturer

Anti-vibration system

Multi-Function Control Handle

Adjustable Support Harness

Shall be used for sanitizing large areas

Shall include pressure pump kit

Shall include one (1) container of 2-cycle engine oil

**ITEM #3, CORDLESS FOGGER/MISTER, 18 VOLT WITH 2.0 AH BATTERY AND CHARGER INCLUDED, RYOBI MODEL #P2850, AS SPECIFIED OR EQUAL**

Weight: 7.2 Lbs.

Sprays over 10,000 sq. ft. per charge

Atomized particles reach up to 15 ft. away

Battery powered

0.5 Gal. chemical tank

3-year warranty

**ITEM #4, CORDLESS HANDHELD AIRLESS DISINFECTANT SPRAYER, SANISPRAY HP 2.0, MANUFACTURED BY GRACO, AS SPECIFIED OR EQUAL**

**COMPLIANCE**

**YES NO**

Battery Capacity (Ah) 2.0

Battery Chemistry Lithium-ion

Battery Voltage (V) 20

Compatible Replacement Pump 19Y967

Frame Configuration Handheld

Included Accessories: RAC X LP 313 Spray Tip, RAC X LP 515

Spray Tip, RAC X LP 619 Spray Tip,

Five (5) - 42 oz. FlexLiner Bags,

Two (2) - DEWALT 20V MAX 2.0 Ah

Lithium Ion Batteries, DEWALT 20V

MAX Battery Charger, Fifteen (15) in Spray

Extension, Flex Liner Storage Plug,

Storage Bag

Maximum Flow Rate (GPM) 0.16

Maximum Tip Size (in) 0.019

Maximum Working Pressure (psi) 1000

Power Source Battery Powered

Pressure Control Type Adjustable

Series 20

Type Handheld Cordless Airless Spray

**OPTION**

**4A. Liner Kit for Cordless Handheld Airless Disinfectant Sprayer,**

**SaniSpray HP 2.0**

**ITEM #5, HANDHELD PORTABLE FOGGER, POWERJOE (SNOW JOE/SUN JOE), MODEL #24V-PS1, AS SPECIFIED OR EQUAL**

Battery Capacity (Ah) 4.0

Interchangeable nozzle connections Yes

Battery Run Time (max) 20

Number of Spray Patterns 3

Battery Voltage (V) 24

Power Type Cordless 24V Battery

Capacity 32 Fl Oz

Weight (lbs) 4.4

**OPTION**

**5A. Extra Battery for Power Joe Model #24V-PS1**

**ITEM #6, MULTI-PURPOSE ADJUSTABLE CONE SPRAYER, CHAPIN MANUFACTURER, AS SPECIFIED, OR EQUAL**

**COMPLIANCE**

**YES NO**

Battery Capacity (Ah) 4.0

Interchangeable nozzle connections Yes

Battery Run Time (max) 20

Number of Spray Patterns 3

Battery Voltage (V) 24

Power Type Cordless 24V Battery

Capacity 32 Fl Oz

Weight (lbs) 4.4